Flush mount MODBUS room thermostat for 2-/4-pipe FCU with on/off outputs and optional electrical heater application, fit for square conduit boxes

Technical details:  
- Operating voltage: AC 230 V  
- Power consumption: 7 VA  
- Setpoint setting range: 5…5 °C  
- Switching differential: 0.5…6 K  
- Communication: Bus: Modbus RTU (RS 485)   
- Analog inputs, number: 2   
- Relay outputs: Fan: Normally open contact , Valve: Normally open contact , Non floating   
- Relay outputs, number: 5   
- Relay output, switching voltage: 230 V  
- Relay output, switching current: 5 (2)A   
- Type of fixing: Recessed rectangular conduit box BS4662 with fixing centres of 60.3 mm   
- Degree of protection: IP30   
- Dimensions (W x H x D): 86 x 86 x 57 mm  
- Color: White   
- Warranty: 24 Months

|  |  |  |  |
| --- | --- | --- | --- |
| Product no. | Stock no. |  | Price |
| RDF302.B | S55770-T416 |  |  |